; Windows Virtual Serial Port Setup File
; Copyright (c) 2002,2003 Huawei Incorporated
; Manufacturer: Huawei Incorporated
;
; This INF file installs a virtual COM port on Win2K system.

[Version]
signature  = "$WINDOWS NT$"
Class      = Ports
Provider   = %HUAWEI%
ClassGuid  = {4D36E978-E325-11CE-BFC1-08002BE10318}
DriverVer  = 12/05/2014,2.00.05.00
CatalogFile = hw_usbvcom.cat


[SourceDisksNames]
1 = %HWSRCDISK%,,,
2 = %HWSRCDISK%,,,

[SourceDisksFiles.x86]
hw_usbvcom.sys = 1

[SourceDisksFiles.amd64]
hw_usbvcom.sys = 2

[ControlFlags]
ExcludeFromSelect = *

[DestinationDirs]
DefaultDestDir = 12

[Manufacturer]
%HUAWEI% = QcomSerialPort, NTx86, NTamd64

[QcomSerialPort.NTx86]
%QcomDevice00% = QportInstall00, USB\VID_12d1&PID_3609
%QcomDevice00% = QportInstall00, USB\VID_12d1&PID_360b&MI_03
%QcomDevice00% = QportInstall00, USB\VID_12d1&PID_360b&MI_02
%QcomDevice00% = QportInstall00, USB\VID_12d1&PID_3613&MI_03
%QcomDevice00% = QportInstall00, USB\VID_12d1&PID_3613&MI_02
%QcomDevice00% = QportInstall00, USB\VID_12d1&PID_3a0b&MI_03
%QcomDevice00% = QportInstall00, USB\VID_12d1&PID_3a0b&MI_02
%QcomDevice00% = QportInstall00, USB\VID_12d1&PID_3a13&MI_03
%QcomDevice00% = QportInstall00, USB\VID_12d1&PID_3a13&MI_02

[QcomSerialPort.NTamd64]
%QcomDevice00% = QportInstall00, USB\VID_12d1&PID_3609
%QcomDevice00% = QportInstall00, USB\VID_12d1&PID_360b&MI_03
%QcomDevice00% = QportInstall00, USB\VID_12d1&PID_360b&MI_02
%QcomDevice00% = QportInstall00, USB\VID_12d1&PID_3613&MI_03
%QcomDevice00% = QportInstall00, USB\VID_12d1&PID_3613&MI_02
%QcomDevice00% = QportInstall00, USB\VID_12d1&PID_3a0b&MI_03
%QcomDevice00% = QportInstall00, USB\VID_12d1&PID_3a0b&MI_02
%QcomDevice00% = QportInstall00, USB\VID_12d1&PID_3a13&MI_03
%QcomDevice00% = QportInstall00, USB\VID_12d1&PID_3a13&MI_02

; ###### Installation Section ######

[QportInstall00]
CopyFiles = CopyFileSection00
AddReg = All00, AddReg

[QportInstall00.Services]
AddService = HSPL_usbvcom,  0x00000002, Qport_Service_Inst00

[Qport_Service_Inst00]
DisplayName   = "HUAWEI USB COM driver"
ServiceType   = 1
StartType     = 3
ErrorControl  = 1
ServiceBinary = %12%\hw_usbvcom.sys

[CopyFileSection00]
hw_usbvcom.sys

[All00]
HKR,,NTMPDriver,,hw_usbvcom.sys
HKR,,PortIdentify,,HWPNP

[AddReg]
HKR,,PortSubClass,1,01
HKR,,EnumPropPages32,,"MsPorts.dll,SerialPortPropPageProvider"

[Strings]
HUAWEI   = "HUAWEI Incorporated"
HWSRCDISK = "HUAWEI COM Diskette"
QcomDevice00 = "HUAWEI USB COM 1.0"


